$**********************************************************
$ (c) 2005 by JVL Industri Elektronik A/S
$
$ EDS File for MAC00-FDx
$**********************************************************



[File]
$ File Description Section:
$   For more information about the meaning of each entry, please check
$   DeviceNet Specification Volume II Chapter 4-3.5.1

    DescText    = "JVL MAC00-FDx DeviceNet module";
    CreateDate  = 02-03-2005;
    CreateTime  = 12:00:00;
    ModDate     = 02-06-2005;
    ModTime     = 12:00:00;
    Revision    = 1.1;
    HomeURL	= "http://www.jvl.dk/files/Downloads/Elektronic datasheets/mac00-fdx.eds";


[Device]
$ Device Description Section:
$   For more information about the meaning of each entry, please check
$   DeviceNet Specification Volume II Chapter 4-3.5.2

    VendCode    = 936;                          $ Identity Object - Vendor ID - JVL Industri Elektronik A/S
    ProdType    = 0x10;                         $ Identity Object - Device Type - Position Controller
    ProdCode    = 1;                            $ Identity Object - Product Code
    MajRev      = 1;                            $ Identity Object - Major Revision
    MinRev      = 1;                            $ Identity Object - Minor Revision
    ProdName    = "MAC00-FDx"; 			$ Identity Object - Product Name

    VendName    = "JVL Industri Elektronik A/S";
    ProdTypeStr = "Position Controller";
    Catalog     = "MAC00-FDx";
    Icon        = "mac00-fdx.ico";   $ Uncomment this if your configurator supports ico files.


[IO_Info]
$ I/O Characteristics Section:
$   For more information about the meaning of each entry, please check
$   DeviceNet Specification Volume II Chapter 4-3.5.3

    Default=0x0001;                         $ default is Poll Only

    PollInfo=
            0x0007,                         $ compatible with all
            1,                              $ Default Input = Input1
            1;                              $ Default Output = Output1

$ Input Connections

    Input1=
            8,                              $ 8 bytes are transfered
            0,                              $ all bits are significant
            0x0001,                         $ Poll
            "Assembly Instance 102",        $ Name
            6, "20 04 24 65 30 03",         $ Assembly Object Instance 101, Attribute 3
            "Asm 102: Position Con, Attr 33";   $ Help (max 30 chars)

$ Output Connections

    Output1=
            8,                              $ 8 bytes are transfered
            0,                              $ all bits are significant
            0x0001,                         $ Poll
            "Assembly Instance 101",        $ Name
            6, "20 04 24 66 30 03",         $ Assembly Object Instance 102, Attribute 3
            "Asm 101: Position con, Attr 32";   $ Help (max 30 chars)



[ParamClass]
$ Parameter Class Section:
$   For more information about the meaning of each entry, please check
$   DeviceNet Specification Volume II Chapter 4-3.5.4 and Chapter 6-14.1

    MaxInst     = 275;                        $ number of parameters supported
    Descriptor  = 1;                        $ supports parameter instances and stub attributes
    CfgAssembly = 0;                        $ not used here


[Params]
$ Parameter Section:
$   For more information about the meaning of each entry, please check
$   DeviceNet Specification Volume II Chapter 4-3.5.5 and Chapter 6-14.2


   Param1=
	0,                              $ parameter value slot
	6, "20 64 24 01 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"PROG_VERSION",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param2=
	0,                              $ parameter value slot
	6, "20 64 24 02 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"MODE_REG",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param3=
	0,                              $ parameter value slot
	6, "20 64 24 03 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_SOLL",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param4=
	0,                              $ parameter value slot
	6, "20 64 24 04 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_NEW",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param5=
	0,                              $ parameter value slot
	6, "20 64 24 05 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"V_SOLL",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param6=
	0,                              $ parameter value slot
	6, "20 64 24 06 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"A_SOLL",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param7=
	0,                              $ parameter value slot
	6, "20 64 24 07 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"T_SOLL",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param8=
	0,                              $ parameter value slot
	6, "20 64 24 08 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_FNC",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param9=
	0,                              $ parameter value slot
	6, "20 64 24 09 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"INDEX_OFFSET",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param10=
	0,                              $ parameter value slot
	6, "20 64 24 0A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_IST",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param11=
	0,                              $ parameter value slot
	6, "20 64 24 0B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"V_IST_16",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param12=
	0,                              $ parameter value slot
	6, "20 64 24 0C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"V_IST",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param13=
	0,                              $ parameter value slot
	6, "20 64 24 0D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"KVOUT",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param14=
	0,                              $ parameter value slot
	6, "20 64 24 0E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"GEARF_1",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param15=
	0,                              $ parameter value slot
	6, "20 64 24 0F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"GEARF_2",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param16=
	0,                              $ parameter value slot
	6, "20 64 24 10 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"I2T",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param17=
	0,                              $ parameter value slot
	6, "20 64 24 11 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"I2TLIM",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param18=
	0,                              $ parameter value slot
	6, "20 64 24 12 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"UIT",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param19=
	0,                              $ parameter value slot
	6, "20 64 24 13 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"UITLIM",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param20=
	0,                              $ parameter value slot
	6, "20 64 24 14 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"FLWERR",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param21=
	0,                              $ parameter value slot
	6, "20 64 24 15 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"U_24V",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param22=
	0,                              $ parameter value slot
	6, "20 64 24 16 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"FLWERRMAX",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param23=
	0,                              $ parameter value slot
	6, "20 64 24 17 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"UV_HANDLE",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param24=
	0,                              $ parameter value slot
	6, "20 64 24 18 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"FNCERR",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param25=
	0,                              $ parameter value slot
	6, "20 64 24 19 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 25",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param26=
	0,                              $ parameter value slot
	6, "20 64 24 1A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"FNCERRMAX",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param27=
	0,                              $ parameter value slot
	6, "20 64 24 1B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"UVMIN",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param28=
	0,                              $ parameter value slot
	6, "20 64 24 1C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"MIN_P_IST",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param29=
	0,                              $ parameter value slot
	6, "20 64 24 1D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"DEGC",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param30=
	0,                              $ parameter value slot
	6, "20 64 24 1E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"MAX_P_IST",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param31=
	0,                              $ parameter value slot
	6, "20 64 24 1F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"DEGCMAX",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param32=
	0,                              $ parameter value slot
	6, "20 64 24 20 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ACC_EMERG",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param33=
	0,                              $ parameter value slot
	6, "20 64 24 21 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"INPOSWIN",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param34=
	0,                              $ parameter value slot
	6, "20 64 24 22 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"INPOSCNT",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param35=
	0,                              $ parameter value slot
	6, "20 64 24 23 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ERR_STAT",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param36=
	0,                              $ parameter value slot
	6, "20 64 24 24 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"CNTRL_BITS",                   $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param37=
	0,                              $ parameter value slot
	6, "20 64 24 25 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"START_MODE",                   $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param38=
	0,                              $ parameter value slot
	6, "20 64 24 26 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_HOME",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param39=
	0,                              $ parameter value slot
	6, "20 64 24 27 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"HW_SETUP",                     $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param40=
	0,                              $ parameter value slot
	6, "20 64 24 28 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"V_HOME",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param41=
	0,                              $ parameter value slot
	6, "20 64 24 29 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"T_HOME",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param42=
	0,                              $ parameter value slot
	6, "20 64 24 2A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"HOME_MODE",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param43=
	0,                              $ parameter value slot
	6, "20 64 24 2B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"P_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param44=
	0,                              $ parameter value slot
	6, "20 64 24 2C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"V_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param45=
	0,                              $ parameter value slot
	6, "20 64 24 2D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"A_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param46=
	0,                              $ parameter value slot
	6, "20 64 24 2E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"T_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param47=
	0,                              $ parameter value slot
	6, "20 64 24 2F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"L_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param48=
	0,                              $ parameter value slot
	6, "20 64 24 30 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Z_REG_P",                      $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param49=
	0,                              $ parameter value slot
	6, "20 64 24 31 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS0",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param50=
	0,                              $ parameter value slot
	6, "20 64 24 32 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 50",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param51=
	0,                              $ parameter value slot
	6, "20 64 24 33 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS1",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param52=
	0,                              $ parameter value slot
	6, "20 64 24 34 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 52",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param53=
	0,                              $ parameter value slot
	6, "20 64 24 35 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS2",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param54=
	0,                              $ parameter value slot
	6, "20 64 24 36 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 54",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param55=
	0,                              $ parameter value slot
	6, "20 64 24 37 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS3",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param56=
	0,                              $ parameter value slot
	6, "20 64 24 38 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 56",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param57=
	0,                              $ parameter value slot
	6, "20 64 24 39 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS4",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param58=
	0,                              $ parameter value slot
	6, "20 64 24 3A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 58",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param59=
	0,                              $ parameter value slot
	6, "20 64 24 3B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS5",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param60=
	0,                              $ parameter value slot
	6, "20 64 24 3C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 60",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param61=
	0,                              $ parameter value slot
	6, "20 64 24 3D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS6",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param62=
	0,                              $ parameter value slot
	6, "20 64 24 3E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 62",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param63=
	0,                              $ parameter value slot
	6, "20 64 24 3F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"POS7",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param64=
	0,                              $ parameter value slot
	6, "20 64 24 40 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 64",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param65=
	0,                              $ parameter value slot
	6, "20 64 24 41 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL0",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param66=
	0,                              $ parameter value slot
	6, "20 64 24 42 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL1",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param67=
	0,                              $ parameter value slot
	6, "20 64 24 43 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL2",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param68=
	0,                              $ parameter value slot
	6, "20 64 24 44 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL3",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param69=
	0,                              $ parameter value slot
	6, "20 64 24 45 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL4",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param70=
	0,                              $ parameter value slot
	6, "20 64 24 46 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL5",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param71=
	0,                              $ parameter value slot
	6, "20 64 24 47 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL6",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param72=
	0,                              $ parameter value slot
	6, "20 64 24 48 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"VEL7",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param73=
	0,                              $ parameter value slot
	6, "20 64 24 49 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ACC0",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param74=
	0,                              $ parameter value slot
	6, "20 64 24 4A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ACC1",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param75=
	0,                              $ parameter value slot
	6, "20 64 24 4B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ACC2",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param76=
	0,                              $ parameter value slot
	6, "20 64 24 4C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ACC3",                         $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param77=
	0,                              $ parameter value slot
	6, "20 64 24 4D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"TQ0",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param78=
	0,                              $ parameter value slot
	6, "20 64 24 4E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"TQ1",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param79=
	0,                              $ parameter value slot
	6, "20 64 24 4F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"TQ2",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param80=
	0,                              $ parameter value slot
	6, "20 64 24 50 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"TQ3",                          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param81=
	0,                              $ parameter value slot
	6, "20 64 24 51 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"LOAD0",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param82=
	0,                              $ parameter value slot
	6, "20 64 24 52 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"LOAD1",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param83=
	0,                              $ parameter value slot
	6, "20 64 24 53 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"LOAD2",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param84=
	0,                              $ parameter value slot
	6, "20 64 24 54 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"LOAD3",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param85=
	0,                              $ parameter value slot
	6, "20 64 24 55 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ZERO0",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param86=
	0,                              $ parameter value slot
	6, "20 64 24 56 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ZERO1",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param87=
	0,                              $ parameter value slot
	6, "20 64 24 57 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ZERO2",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param88=
	0,                              $ parameter value slot
	6, "20 64 24 58 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"ZERO3",                        $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param89=
	0,                              $ parameter value slot
	6, "20 64 24 59 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 89",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param90=
	0,                              $ parameter value slot
	6, "20 64 24 5A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 90",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param91=
	0,                              $ parameter value slot
	6, "20 64 24 5B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 91",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param92=
	0,                              $ parameter value slot
	6, "20 64 24 5C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 92",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param93=
	0,                              $ parameter value slot
	6, "20 64 24 5D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 93",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param94=
	0,                              $ parameter value slot
	6, "20 64 24 5E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 94",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param95=
	0,                              $ parameter value slot
	6, "20 64 24 5F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 95",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param96=
	0,                              $ parameter value slot
	6, "20 64 24 60 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 96",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param97=
	0,                              $ parameter value slot
	6, "20 64 24 61 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 97",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param98=
	0,                              $ parameter value slot
	6, "20 64 24 62 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 98",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param99=
	0,                              $ parameter value slot
	6, "20 64 24 63 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 99",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param100=
	0,                              $ parameter value slot
	6, "20 64 24 64 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 100",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param101=
	0,                              $ parameter value slot
	6, "20 64 24 65 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 101",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param102=
	0,                              $ parameter value slot
	6, "20 64 24 66 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 102",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param103=
	0,                              $ parameter value slot
	6, "20 64 24 67 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 103",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param104=
	0,                              $ parameter value slot
	6, "20 64 24 68 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 104",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param105=
	0,                              $ parameter value slot
	6, "20 64 24 69 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 105",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param106=
	0,                              $ parameter value slot
	6, "20 64 24 6A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 106",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param107=
	0,                              $ parameter value slot
	6, "20 64 24 6B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 107",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param108=
	0,                              $ parameter value slot
	6, "20 64 24 6C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 108",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param109=
	0,                              $ parameter value slot
	6, "20 64 24 6D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 109",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param110=
	0,                              $ parameter value slot
	6, "20 64 24 6E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 110",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param111=
	0,                              $ parameter value slot
	6, "20 64 24 6F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 111",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param112=
	0,                              $ parameter value slot
	6, "20 64 24 70 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 112",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param113=
	0,                              $ parameter value slot
	6, "20 64 24 71 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 113",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param114=
	0,                              $ parameter value slot
	6, "20 64 24 72 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 114",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param115=
	0,                              $ parameter value slot
	6, "20 64 24 73 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 115",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param116=
	0,                              $ parameter value slot
	6, "20 64 24 74 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 116",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param117=
	0,                              $ parameter value slot
	6, "20 64 24 75 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 117",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param118=
	0,                              $ parameter value slot
	6, "20 64 24 76 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 118",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param119=
	0,                              $ parameter value slot
	6, "20 64 24 77 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 119",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param120=
	0,                              $ parameter value slot
	6, "20 64 24 78 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 120",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param121=
	0,                              $ parameter value slot
	6, "20 64 24 79 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 121",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param122=
	0,                              $ parameter value slot
	6, "20 64 24 7A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 122",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param123=
	0,                              $ parameter value slot
	6, "20 64 24 7B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 123",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param124=
	0,                              $ parameter value slot
	6, "20 64 24 7C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 124",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param125=
	0,                              $ parameter value slot
	6, "20 64 24 7D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 125",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param126=
	0,                              $ parameter value slot
	6, "20 64 24 7E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 126",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param127=
	0,                              $ parameter value slot
	6, "20 64 24 7F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 127",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param128=
	0,                              $ parameter value slot
	6, "20 64 24 80 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 128",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param129=
	0,                              $ parameter value slot
	6, "20 64 24 81 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 129",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param130=
	0,                              $ parameter value slot
	6, "20 64 24 82 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 130",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param131=
	0,                              $ parameter value slot
	6, "20 64 24 83 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 131",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param132=
	0,                              $ parameter value slot
	6, "20 64 24 84 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 132",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param133=
	0,                              $ parameter value slot
	6, "20 64 24 85 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 133",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param134=
	0,                              $ parameter value slot
	6, "20 64 24 86 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 134",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param135=
	0,                              $ parameter value slot
	6, "20 64 24 87 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 135",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param136=
	0,                              $ parameter value slot
	6, "20 64 24 88 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 136",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param137=
	0,                              $ parameter value slot
	6, "20 64 24 89 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 137",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param138=
	0,                              $ parameter value slot
	6, "20 64 24 8A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 138",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param139=
	0,                              $ parameter value slot
	6, "20 64 24 8B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 139",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param140=
	0,                              $ parameter value slot
	6, "20 64 24 8C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 140",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param141=
	0,                              $ parameter value slot
	6, "20 64 24 8D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 141",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param142=
	0,                              $ parameter value slot
	6, "20 64 24 8E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 142",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param143=
	0,                              $ parameter value slot
	6, "20 64 24 8F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 143",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param144=
	0,                              $ parameter value slot
	6, "20 64 24 90 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 144",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param145=
	0,                              $ parameter value slot
	6, "20 64 24 91 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 145",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param146=
	0,                              $ parameter value slot
	6, "20 64 24 92 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 146",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param147=
	0,                              $ parameter value slot
	6, "20 64 24 93 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 147",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param148=
	0,                              $ parameter value slot
	6, "20 64 24 94 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 148",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param149=
	0,                              $ parameter value slot
	6, "20 64 24 95 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 149",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param150=
	0,                              $ parameter value slot
	6, "20 64 24 96 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 150",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param151=
	0,                              $ parameter value slot
	6, "20 64 24 97 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 151",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param152=
	0,                              $ parameter value slot
	6, "20 64 24 98 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 152",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param153=
	0,                              $ parameter value slot
	6, "20 64 24 99 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 153",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param154=
	0,                              $ parameter value slot
	6, "20 64 24 9A 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 154",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param155=
	0,                              $ parameter value slot
	6, "20 64 24 9B 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 155",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param156=
	0,                              $ parameter value slot
	6, "20 64 24 9C 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 156",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param157=
	0,                              $ parameter value slot
	6, "20 64 24 9D 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 157",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param158=
	0,                              $ parameter value slot
	6, "20 64 24 9E 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 158",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param159=
	0,                              $ parameter value slot
	6, "20 64 24 9F 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 159",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param160=
	0,                              $ parameter value slot
	6, "20 64 24 A0 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 160",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param161=
	0,                              $ parameter value slot
	6, "20 64 24 A1 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 161",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param162=
	0,                              $ parameter value slot
	6, "20 64 24 A2 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 162",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param163=
	0,                              $ parameter value slot
	6, "20 64 24 A3 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 163",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param164=
	0,                              $ parameter value slot
	6, "20 64 24 A4 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 164",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param165=
	0,                              $ parameter value slot
	6, "20 64 24 A5 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 165",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param166=
	0,                              $ parameter value slot
	6, "20 64 24 A6 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 166",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param167=
	0,                              $ parameter value slot
	6, "20 64 24 A7 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 167",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param168=
	0,                              $ parameter value slot
	6, "20 64 24 A8 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 168",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param169=
	0,                              $ parameter value slot
	6, "20 64 24 A9 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 169",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param170=
	0,                              $ parameter value slot
	6, "20 64 24 AA 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 170",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param171=
	0,                              $ parameter value slot
	6, "20 64 24 AB 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 171",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param172=
	0,                              $ parameter value slot
	6, "20 64 24 AC 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 172",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param173=
	0,                              $ parameter value slot
	6, "20 64 24 AD 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 173",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param174=
	0,                              $ parameter value slot
	6, "20 64 24 AE 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 174",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param175=
	0,                              $ parameter value slot
	6, "20 64 24 AF 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 175",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param176=
	0,                              $ parameter value slot
	6, "20 64 24 B0 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 176",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param177=
	0,                              $ parameter value slot
	6, "20 64 24 B1 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 177",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param178=
	0,                              $ parameter value slot
	6, "20 64 24 B2 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 178",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param179=
	0,                              $ parameter value slot
	6, "20 64 24 B3 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 179",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param180=
	0,                              $ parameter value slot
	6, "20 64 24 B4 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 180",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param181=
	0,                              $ parameter value slot
	6, "20 64 24 B5 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 181",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param182=
	0,                              $ parameter value slot
	6, "20 64 24 B6 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 182",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param183=
	0,                              $ parameter value slot
	6, "20 64 24 B7 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 183",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param184=
	0,                              $ parameter value slot
	6, "20 64 24 B8 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 184",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param185=
	0,                              $ parameter value slot
	6, "20 64 24 B9 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 185",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param186=
	0,                              $ parameter value slot
	6, "20 64 24 BA 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 186",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param187=
	0,                              $ parameter value slot
	6, "20 64 24 BB 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 187",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param188=
	0,                              $ parameter value slot
	6, "20 64 24 BC 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 188",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param189=
	0,                              $ parameter value slot
	6, "20 64 24 BD 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 189",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param190=
	0,                              $ parameter value slot
	6, "20 64 24 BE 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 190",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param191=
	0,                              $ parameter value slot
	6, "20 64 24 BF 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 191",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param192=
	0,                              $ parameter value slot
	6, "20 64 24 C0 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 192",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param193=
	0,                              $ parameter value slot
	6, "20 64 24 C1 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 193",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param194=
	0,                              $ parameter value slot
	6, "20 64 24 C2 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 194",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param195=
	0,                              $ parameter value slot
	6, "20 64 24 C3 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 195",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param196=
	0,                              $ parameter value slot
	6, "20 64 24 C4 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 196",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param197=
	0,                              $ parameter value slot
	6, "20 64 24 C5 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 197",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param198=
	0,                              $ parameter value slot
	6, "20 64 24 C6 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 198",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param199=
	0,                              $ parameter value slot
	6, "20 64 24 C7 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 199",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param200=
	0,                              $ parameter value slot
	6, "20 64 24 C8 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 200",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param201=
	0,                              $ parameter value slot
	6, "20 64 24 C9 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 201",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param202=
	0,                              $ parameter value slot
	6, "20 64 24 CA 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 202",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param203=
	0,                              $ parameter value slot
	6, "20 64 24 CB 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 203",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param204=
	0,                              $ parameter value slot
	6, "20 64 24 CC 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 204",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param205=
	0,                              $ parameter value slot
	6, "20 64 24 CD 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 205",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param206=
	0,                              $ parameter value slot
	6, "20 64 24 CE 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 206",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param207=
	0,                              $ parameter value slot
	6, "20 64 24 CF 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 207",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param208=
	0,                              $ parameter value slot
	6, "20 64 24 D0 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 208",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param209=
	0,                              $ parameter value slot
	6, "20 64 24 D1 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 209",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param210=
	0,                              $ parameter value slot
	6, "20 64 24 D2 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 210",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param211=
	0,                              $ parameter value slot
	6, "20 64 24 D3 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 211",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param212=
	0,                              $ parameter value slot
	6, "20 64 24 D4 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 212",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param213=
	0,                              $ parameter value slot
	6, "20 64 24 D5 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 213",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param214=
	0,                              $ parameter value slot
	6, "20 64 24 D6 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 214",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param215=
	0,                              $ parameter value slot
	6, "20 64 24 D7 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 215",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param216=
	0,                              $ parameter value slot
	6, "20 64 24 D8 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 216",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param217=
	0,                              $ parameter value slot
	6, "20 64 24 D9 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 217",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param218=
	0,                              $ parameter value slot
	6, "20 64 24 DA 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 218",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param219=
	0,                              $ parameter value slot
	6, "20 64 24 DB 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 219",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param220=
	0,                              $ parameter value slot
	6, "20 64 24 DC 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 220",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param221=
	0,                              $ parameter value slot
	6, "20 64 24 DD 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 221",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param222=
	0,                              $ parameter value slot
	6, "20 64 24 DE 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 222",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param223=
	0,                              $ parameter value slot
	6, "20 64 24 DF 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 223",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param224=
	0,                              $ parameter value slot
	6, "20 64 24 E0 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 224",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param225=
	0,                              $ parameter value slot
	6, "20 64 24 E1 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 225",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param226=
	0,                              $ parameter value slot
	6, "20 64 24 E2 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 226",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param227=
	0,                              $ parameter value slot
	6, "20 64 24 E3 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 227",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param228=
	0,                              $ parameter value slot
	6, "20 64 24 E4 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 228",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param229=
	0,                              $ parameter value slot
	6, "20 64 24 E5 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 229",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param230=
	0,                              $ parameter value slot
	6, "20 64 24 E6 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 230",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param231=
	0,                              $ parameter value slot
	6, "20 64 24 E7 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 231",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param232=
	0,                              $ parameter value slot
	6, "20 64 24 E8 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 232",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param233=
	0,                              $ parameter value slot
	6, "20 64 24 E9 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 233",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param234=
	0,                              $ parameter value slot
	6, "20 64 24 EA 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 234",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param235=
	0,                              $ parameter value slot
	6, "20 64 24 EB 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 235",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param236=
	0,                              $ parameter value slot
	6, "20 64 24 EC 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 236",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param237=
	0,                              $ parameter value slot
	6, "20 64 24 ED 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 237",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param238=
	0,                              $ parameter value slot
	6, "20 64 24 EE 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 238",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision


   Param239=
	0,                              $ parameter value slot
	6, "20 64 24 EF 30 01",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Motor parameter 239",          $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647, 0,     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param240=
	0,                              $ parameter value slot
	6, "20 65 24 01 30 03",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Inputs",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0x3F, 0,                     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param241=
	0,                              $ parameter value slot
	6, "20 65 24 01 30 04",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Outputs",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0x3, 0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param242=
	0,                              $ parameter value slot
	6, "20 65 24 01 30 05",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Input Active Level",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0x3F, 0,                     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param243=
	0,                              $ parameter value slot
	6, "20 65 24 01 30 06",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Input setup",                  $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0x3F, 0,                     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param244=
	0,                              $ parameter value slot
	6, "20 65 24 01 30 07",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Output setup",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0x03, 0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param245=
	0,                              $ parameter value slot
	6, "20 65 24 02 30 03",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Motor status",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0xff, 0,                     $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param246=
	0,                              $ parameter value slot
	6, "20 65 24 03 30 03",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xD1, 1,                        $ type is BYTE, length is 1 byte
	"Module setup",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 0xff, 0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param247=
	0,                              $ parameter value slot
	6, "20 65 24 03 30 04",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC6, 1,                        $ type is USINT, length is 1 byte
	"Execute FastMac",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 255, 0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param248=
	0,                              $ parameter value slot
	6, "20 65 24 03 30 05",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC6, 1,                        $ type is USINT, length is 1 byte
	"Module command",               $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 255, 0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param256=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 03",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC6, 1,                        $ type is USINT, length is 1 byte
	"Operating Mode",               $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 2, 0,                        $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param257=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 06",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Target position",               $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param258=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 07",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Target velocity",              $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,6827,   $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param259=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 08",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Acceleration",                 $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,341444,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param260=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 0A",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Incremental position",         $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param261=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 0B",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Load data",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param262=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 0C",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"On Target Position",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param263=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 0D",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Actual Position",              $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param264=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 0E",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Actual Velocity",              $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param265=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 11",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Enable",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param266=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 14",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Smooth Stop",                  $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param267=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 15",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Hard Stop",                    $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param268=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 19",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Torque",                       $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 1023,0,                      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param269=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 2D",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Max Dynamic Following Error",  $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 2147483647,0,                $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param270=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 30",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Actual Following Error",       $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param271=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 31",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC6, 1,                        $ type is USINT, length is 1 byte
	"Hard Limit Action",            $ parameter name
	"",                             $ units string
	"",                             $ help string
	0, 2, 0,                        $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param272=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 34",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Soft Limit Enable",            $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param273=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 36",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Positive Soft Limit Position", $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param274=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 37",         $ link path size and path
	0x20,                           $ descriptor: monitor parameter
	0xC4, 4,                        $ type is DINT, length is 4 byte
	"Negative Soft Limit Position", $ parameter name
	"",                             $ units string
	"",                             $ help string
	-2147483648, 2147483647,0,      $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision

   Param275=
	0,                              $ parameter value slot
	6, "20 25 24 01 30 3A",         $ link path size and path
	0x30,                           $ descriptor: monitor parameter, read only
	0xC1, 1,                        $ type is BOOL, length is 1 byte
	"Load Data Complete",           $ parameter name
	"",                             $ units string
	"",                             $ help string
	0,1,0,                          $ min, max, default
	1, 1, 1, 0,                     $ mult, div, base, offset scaling
	0, 0, 0, 0, 0 ;                 $ scaling links and precision





[EnumPar]
	Param240= "IN1","IN2","IN3","IN4","NL","PL";
	Param241= "OUT1","OUT2";
	Param242= "IN1","IN2","IN3","IN4","NL","PL";
	Param243= "IN1","IN2","IN3","IN4","NL","PL";
	Param244= "OUT1","OUT2";
	Param245= "Motor error","Disconnected","Limit switch","Reserved","In position","Acceleration","Decceleration","Reserved";
	Param246= "Reserved","Reserved","Reserved","Reserved","Reserved","Reserved","Set Vel=0 on error","Endless relative";

	Param256= "Position mode","Velocity mode", "Torque mode";

	Param271 = "Output off","Hard Stop", "Smooth Stop";

[Groups]
	Group1 = "Motor parameters", 239,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15,
                                     16,17,18,19,20,21,22,23,24,25,26,27,28,
                                     29,30,31,32,33,34,35,36,37,38,39,40,41,
                                     42,43,44,45,46,47,48,49,50,51,52,53,54,
                                     55,56,57,58,59,60,61,62,63,64,65,66,67,
				     68,69,70,71,72,73,74,75,76,77,78,79,80,
                                     81,82,83,84,85,86,87,88,89,90,91,92,93,
                                     94,95,96,97,98,99,100,101,102,103,104,
                                     105,106,107,108,109,110,111,112,113,114,
                                     115,116,117,118,119,120,121,122,123,124,
                                     125,126,127,128,129,130,131,132,133,134,
                                     135,136,137,138,139,140,141,142,143,144,
                                     145,146,147,148,149,150,151,152,153,154,
                                     155,156,157,158,159,160,161,162,163,164,
                                     165,166,167,168,169,170,171,172,173,174,
                                     175,176,177,178,179,180,181,182,183,184,
                                     185,186,187,188,189,190,191,192,193,194,
                                     195,196,197,198,199,200,201,202,203,204,
                                     205,206,207,208,209,210,211,212,213,214,
                                     215,216,217,218,219,220,221,222,223,224,
                                     225,226,227,228,229,230,231,232,233,234,
                                     235,236,237,238,239;

	Group2 = "I/O Parameters",   5,240,241,242,243,244;

	Group3 = "Status",	     1,245;

	Group4 = "Commands/Setup",   3,246,247,248;

	Group5 = "Position Controller",
                                     20,256,257,258,259,260,261,262,263,264,265,266,267,268,269,270,271,272,273,274,275;



$ End of File
