$ EZ-EDS Version 3.11 (Beta, May-09, 2012) Generated Electronic Data Sheet

$ ****************************************************************************
$  
$ File:   HILSCHER NETX50-RE_EIS.EDS
$  
$ Author: Ralf Hornung, Hilscher GmbH, Hattersheim, Germany
$         hotline@hilscher.com
$ Date:   20.08.06
$  
$ ****************************************************************************
$  
$ ATTENTION:
$  
$  Changes in this file can cause configuration or communication problems.
$  
$ ****************************************************************************
$  
$ Changes:
$  
$  Version  Date       Name   Description
$ -------------------------------------------------------------------------
$  
$  1.0      20.08.060   RalfH  created
$  
$ ****************************************************************************

[File]
        DescText = "EDS-file for the JVL MAC00-EIx Ethernet/IP module";
        CreateDate = 12-16-2010;
        CreateTime = 10:26:24;
        ModDate = 04-24-2013;
        ModTime = 16:32:10;
        Revision = 1.0;
        HomeURL = "www.jvl.dk";


[Device]
        VendCode = 936;
        VendName = "JVL A/S";
        ProdType = 12;
        ProdTypeStr = "Communications Adapter";
        ProdCode = 1;
        MajRev = 3;
        MinRev = 24;
        ProdName = "MAC00-EIx";
        Catalog = "MAC00-EIx";

$  Icon        = "netX_50-RE.ico";

[Device Classification]
        Class1 = EtherNetIP;


[Params]


        Param1 =
                0,                      $ parameter value slot
                6,"20 64 24 01 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "PROG_VERSION",         $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param2 =
                0,                      $ parameter value slot
                6,"20 64 24 02 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "MODE_REG",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param3 =
                0,                      $ parameter value slot
                6,"20 64 24 03 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_SOLL",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param4 =
                0,                      $ parameter value slot
                6,"20 64 24 04 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_NEW",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param5 =
                0,                      $ parameter value slot
                6,"20 64 24 05 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "V_SOLL",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param6 =
                0,                      $ parameter value slot
                6,"20 64 24 06 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "A_SOLL",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param7 =
                0,                      $ parameter value slot
                6,"20 64 24 07 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "T_SOLL",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param8 =
                0,                      $ parameter value slot
                6,"20 64 24 08 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_FNC",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param9 =
                0,                      $ parameter value slot
                6,"20 64 24 09 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "INDEX_OFFSET",         $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param10 =
                0,                      $ parameter value slot
                6,"20 64 24 0A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_IST",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param11 =
                0,                      $ parameter value slot
                6,"20 64 24 0B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "V_IST_16",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param12 =
                0,                      $ parameter value slot
                6,"20 64 24 0C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "V_IST",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param13 =
                0,                      $ parameter value slot
                6,"20 64 24 0D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "KVOUT",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param14 =
                0,                      $ parameter value slot
                6,"20 64 24 0E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "GEARF_1",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param15 =
                0,                      $ parameter value slot
                6,"20 64 24 0F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "GEARF_2",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param16 =
                0,                      $ parameter value slot
                6,"20 64 24 10 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "I2T",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param17 =
                0,                      $ parameter value slot
                6,"20 64 24 11 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "I2TLIM",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param18 =
                0,                      $ parameter value slot
                6,"20 64 24 12 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "UIT",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param19 =
                0,                      $ parameter value slot
                6,"20 64 24 13 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "UITLIM",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param20 =
                0,                      $ parameter value slot
                6,"20 64 24 14 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "FLWERR",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param21 =
                0,                      $ parameter value slot
                6,"20 64 24 15 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "U_24V",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param22 =
                0,                      $ parameter value slot
                6,"20 64 24 16 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "FLWERRMAX",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param23 =
                0,                      $ parameter value slot
                6,"20 64 24 17 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "UV_HANDLE",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param24 =
                0,                      $ parameter value slot
                6,"20 64 24 18 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "FNCERR",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param25 =
                0,                      $ parameter value slot
                6,"20 64 24 19 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 25",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param26 =
                0,                      $ parameter value slot
                6,"20 64 24 1A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "FNCERRMAX",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param27 =
                0,                      $ parameter value slot
                6,"20 64 24 1B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "UVMIN",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param28 =
                0,                      $ parameter value slot
                6,"20 64 24 1C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "MIN_P_IST",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param29 =
                0,                      $ parameter value slot
                6,"20 64 24 1D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "DEGC",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param30 =
                0,                      $ parameter value slot
                6,"20 64 24 1E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "MAX_P_IST",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param31 =
                0,                      $ parameter value slot
                6,"20 64 24 1F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "DEGCMAX",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param32 =
                0,                      $ parameter value slot
                6,"20 64 24 20 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ACC_EMERG",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param33 =
                0,                      $ parameter value slot
                6,"20 64 24 21 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "INPOSWIN",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param34 =
                0,                      $ parameter value slot
                6,"20 64 24 22 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "INPOSCNT",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param35 =
                0,                      $ parameter value slot
                6,"20 64 24 23 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ERR_STAT",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param36 =
                0,                      $ parameter value slot
                6,"20 64 24 24 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "CNTRL_BITS",           $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param37 =
                0,                      $ parameter value slot
                6,"20 64 24 25 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "START_MODE",           $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param38 =
                0,                      $ parameter value slot
                6,"20 64 24 26 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_HOME",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param39 =
                0,                      $ parameter value slot
                6,"20 64 24 27 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "HW_SETUP",             $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param40 =
                0,                      $ parameter value slot
                6,"20 64 24 28 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "V_HOME",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param41 =
                0,                      $ parameter value slot
                6,"20 64 24 29 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "T_HOME",               $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param42 =
                0,                      $ parameter value slot
                6,"20 64 24 2A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "HOME_MODE",            $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param43 =
                0,                      $ parameter value slot
                6,"20 64 24 2B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "P_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param44 =
                0,                      $ parameter value slot
                6,"20 64 24 2C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "V_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param45 =
                0,                      $ parameter value slot
                6,"20 64 24 2D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "A_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param46 =
                0,                      $ parameter value slot
                6,"20 64 24 2E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "T_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param47 =
                0,                      $ parameter value slot
                6,"20 64 24 2F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "L_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param48 =
                0,                      $ parameter value slot
                6,"20 64 24 30 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Z_REG_P",              $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param49 =
                0,                      $ parameter value slot
                6,"20 64 24 31 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS0",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param50 =
                0,                      $ parameter value slot
                6,"20 64 24 32 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 50",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param51 =
                0,                      $ parameter value slot
                6,"20 64 24 33 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS1",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param52 =
                0,                      $ parameter value slot
                6,"20 64 24 34 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 52",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param53 =
                0,                      $ parameter value slot
                6,"20 64 24 35 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS2",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param54 =
                0,                      $ parameter value slot
                6,"20 64 24 36 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 54",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param55 =
                0,                      $ parameter value slot
                6,"20 64 24 37 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS3",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param56 =
                0,                      $ parameter value slot
                6,"20 64 24 38 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 56",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param57 =
                0,                      $ parameter value slot
                6,"20 64 24 39 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS4",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param58 =
                0,                      $ parameter value slot
                6,"20 64 24 3A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 58",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param59 =
                0,                      $ parameter value slot
                6,"20 64 24 3B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS5",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param60 =
                0,                      $ parameter value slot
                6,"20 64 24 3C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 60",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param61 =
                0,                      $ parameter value slot
                6,"20 64 24 3D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS6",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param62 =
                0,                      $ parameter value slot
                6,"20 64 24 3E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 62",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param63 =
                0,                      $ parameter value slot
                6,"20 64 24 3F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "POS7",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param64 =
                0,                      $ parameter value slot
                6,"20 64 24 40 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 64",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param65 =
                0,                      $ parameter value slot
                6,"20 64 24 41 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL0",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param66 =
                0,                      $ parameter value slot
                6,"20 64 24 42 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL1",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param67 =
                0,                      $ parameter value slot
                6,"20 64 24 43 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL2",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param68 =
                0,                      $ parameter value slot
                6,"20 64 24 44 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL3",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param69 =
                0,                      $ parameter value slot
                6,"20 64 24 45 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL4",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param70 =
                0,                      $ parameter value slot
                6,"20 64 24 46 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL5",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param71 =
                0,                      $ parameter value slot
                6,"20 64 24 47 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL6",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param72 =
                0,                      $ parameter value slot
                6,"20 64 24 48 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "VEL7",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param73 =
                0,                      $ parameter value slot
                6,"20 64 24 49 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ACC0",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param74 =
                0,                      $ parameter value slot
                6,"20 64 24 4A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ACC1",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param75 =
                0,                      $ parameter value slot
                6,"20 64 24 4B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ACC2",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param76 =
                0,                      $ parameter value slot
                6,"20 64 24 4C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ACC3",                 $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param77 =
                0,                      $ parameter value slot
                6,"20 64 24 4D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "TQ0",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param78 =
                0,                      $ parameter value slot
                6,"20 64 24 4E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "TQ1",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param79 =
                0,                      $ parameter value slot
                6,"20 64 24 4F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "TQ2",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param80 =
                0,                      $ parameter value slot
                6,"20 64 24 50 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "TQ3",                  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param81 =
                0,                      $ parameter value slot
                6,"20 64 24 51 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "LOAD0",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param82 =
                0,                      $ parameter value slot
                6,"20 64 24 52 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "LOAD1",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param83 =
                0,                      $ parameter value slot
                6,"20 64 24 53 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "LOAD2",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param84 =
                0,                      $ parameter value slot
                6,"20 64 24 54 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "LOAD3",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param85 =
                0,                      $ parameter value slot
                6,"20 64 24 55 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ZERO0",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param86 =
                0,                      $ parameter value slot
                6,"20 64 24 56 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ZERO1",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param87 =
                0,                      $ parameter value slot
                6,"20 64 24 57 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ZERO2",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param88 =
                0,                      $ parameter value slot
                6,"20 64 24 58 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "ZERO3",                $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param89 =
                0,                      $ parameter value slot
                6,"20 64 24 59 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 89",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param90 =
                0,                      $ parameter value slot
                6,"20 64 24 5A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 90",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param91 =
                0,                      $ parameter value slot
                6,"20 64 24 5B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 91",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param92 =
                0,                      $ parameter value slot
                6,"20 64 24 5C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 92",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param93 =
                0,                      $ parameter value slot
                6,"20 64 24 5D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 93",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param94 =
                0,                      $ parameter value slot
                6,"20 64 24 5E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 94",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param95 =
                0,                      $ parameter value slot
                6,"20 64 24 5F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 95",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param96 =
                0,                      $ parameter value slot
                6,"20 64 24 60 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 96",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param97 =
                0,                      $ parameter value slot
                6,"20 64 24 61 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 97",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param98 =
                0,                      $ parameter value slot
                6,"20 64 24 62 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 98",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param99 =
                0,                      $ parameter value slot
                6,"20 64 24 63 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 99",   $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param100 =
                0,                      $ parameter value slot
                6,"20 64 24 64 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 100",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param101 =
                0,                      $ parameter value slot
                6,"20 64 24 65 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 101",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param102 =
                0,                      $ parameter value slot
                6,"20 64 24 66 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 102",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param103 =
                0,                      $ parameter value slot
                6,"20 64 24 67 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 103",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param104 =
                0,                      $ parameter value slot
                6,"20 64 24 68 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 104",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param105 =
                0,                      $ parameter value slot
                6,"20 64 24 69 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 105",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param106 =
                0,                      $ parameter value slot
                6,"20 64 24 6A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 106",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param107 =
                0,                      $ parameter value slot
                6,"20 64 24 6B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 107",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param108 =
                0,                      $ parameter value slot
                6,"20 64 24 6C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 108",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param109 =
                0,                      $ parameter value slot
                6,"20 64 24 6D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 109",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param110 =
                0,                      $ parameter value slot
                6,"20 64 24 6E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 110",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param111 =
                0,                      $ parameter value slot
                6,"20 64 24 6F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 111",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param112 =
                0,                      $ parameter value slot
                6,"20 64 24 70 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 112",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param113 =
                0,                      $ parameter value slot
                6,"20 64 24 71 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 113",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param114 =
                0,                      $ parameter value slot
                6,"20 64 24 72 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 114",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param115 =
                0,                      $ parameter value slot
                6,"20 64 24 73 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 115",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param116 =
                0,                      $ parameter value slot
                6,"20 64 24 74 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 116",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param117 =
                0,                      $ parameter value slot
                6,"20 64 24 75 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 117",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param118 =
                0,                      $ parameter value slot
                6,"20 64 24 76 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 118",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param119 =
                0,                      $ parameter value slot
                6,"20 64 24 77 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 119",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param120 =
                0,                      $ parameter value slot
                6,"20 64 24 78 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 120",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param121 =
                0,                      $ parameter value slot
                6,"20 64 24 79 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 121",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param122 =
                0,                      $ parameter value slot
                6,"20 64 24 7A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 122",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param123 =
                0,                      $ parameter value slot
                6,"20 64 24 7B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 123",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param124 =
                0,                      $ parameter value slot
                6,"20 64 24 7C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 124",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param125 =
                0,                      $ parameter value slot
                6,"20 64 24 7D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 125",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param126 =
                0,                      $ parameter value slot
                6,"20 64 24 7E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 126",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param127 =
                0,                      $ parameter value slot
                6,"20 64 24 7F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 127",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param128 =
                0,                      $ parameter value slot
                6,"20 64 24 80 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 128",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param129 =
                0,                      $ parameter value slot
                6,"20 64 24 81 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 129",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param130 =
                0,                      $ parameter value slot
                6,"20 64 24 82 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 130",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param131 =
                0,                      $ parameter value slot
                6,"20 64 24 83 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 131",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param132 =
                0,                      $ parameter value slot
                6,"20 64 24 84 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 132",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param133 =
                0,                      $ parameter value slot
                6,"20 64 24 85 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 133",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param134 =
                0,                      $ parameter value slot
                6,"20 64 24 86 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 134",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param135 =
                0,                      $ parameter value slot
                6,"20 64 24 87 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 135",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param136 =
                0,                      $ parameter value slot
                6,"20 64 24 88 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 136",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param137 =
                0,                      $ parameter value slot
                6,"20 64 24 89 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 137",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param138 =
                0,                      $ parameter value slot
                6,"20 64 24 8A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 138",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param139 =
                0,                      $ parameter value slot
                6,"20 64 24 8B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 139",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param140 =
                0,                      $ parameter value slot
                6,"20 64 24 8C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 140",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param141 =
                0,                      $ parameter value slot
                6,"20 64 24 8D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 141",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param142 =
                0,                      $ parameter value slot
                6,"20 64 24 8E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 142",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param143 =
                0,                      $ parameter value slot
                6,"20 64 24 8F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 143",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param144 =
                0,                      $ parameter value slot
                6,"20 64 24 90 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 144",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param145 =
                0,                      $ parameter value slot
                6,"20 64 24 91 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 145",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param146 =
                0,                      $ parameter value slot
                6,"20 64 24 92 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 146",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param147 =
                0,                      $ parameter value slot
                6,"20 64 24 93 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 147",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param148 =
                0,                      $ parameter value slot
                6,"20 64 24 94 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 148",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param149 =
                0,                      $ parameter value slot
                6,"20 64 24 95 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 149",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param150 =
                0,                      $ parameter value slot
                6,"20 64 24 96 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 150",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param151 =
                0,                      $ parameter value slot
                6,"20 64 24 97 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 151",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param152 =
                0,                      $ parameter value slot
                6,"20 64 24 98 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 152",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param153 =
                0,                      $ parameter value slot
                6,"20 64 24 99 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 153",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param154 =
                0,                      $ parameter value slot
                6,"20 64 24 9A 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 154",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param155 =
                0,                      $ parameter value slot
                6,"20 64 24 9B 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 155",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param156 =
                0,                      $ parameter value slot
                6,"20 64 24 9C 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 156",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param157 =
                0,                      $ parameter value slot
                6,"20 64 24 9D 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 157",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param158 =
                0,                      $ parameter value slot
                6,"20 64 24 9E 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 158",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param159 =
                0,                      $ parameter value slot
                6,"20 64 24 9F 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 159",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param160 =
                0,                      $ parameter value slot
                6,"20 64 24 A0 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 160",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param161 =
                0,                      $ parameter value slot
                6,"20 64 24 A1 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 161",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param162 =
                0,                      $ parameter value slot
                6,"20 64 24 A2 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 162",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param163 =
                0,                      $ parameter value slot
                6,"20 64 24 A3 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 163",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param164 =
                0,                      $ parameter value slot
                6,"20 64 24 A4 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 164",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param165 =
                0,                      $ parameter value slot
                6,"20 64 24 A5 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 165",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param166 =
                0,                      $ parameter value slot
                6,"20 64 24 A6 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 166",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param167 =
                0,                      $ parameter value slot
                6,"20 64 24 A7 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 167",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param168 =
                0,                      $ parameter value slot
                6,"20 64 24 A8 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 168",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param169 =
                0,                      $ parameter value slot
                6,"20 64 24 A9 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 169",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param170 =
                0,                      $ parameter value slot
                6,"20 64 24 AA 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 170",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param171 =
                0,                      $ parameter value slot
                6,"20 64 24 AB 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 171",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param172 =
                0,                      $ parameter value slot
                6,"20 64 24 AC 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 172",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param173 =
                0,                      $ parameter value slot
                6,"20 64 24 AD 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 173",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param174 =
                0,                      $ parameter value slot
                6,"20 64 24 AE 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 174",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param175 =
                0,                      $ parameter value slot
                6,"20 64 24 AF 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 175",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param176 =
                0,                      $ parameter value slot
                6,"20 64 24 B0 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 176",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param177 =
                0,                      $ parameter value slot
                6,"20 64 24 B1 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 177",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param178 =
                0,                      $ parameter value slot
                6,"20 64 24 B2 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 178",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param179 =
                0,                      $ parameter value slot
                6,"20 64 24 B3 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 179",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param180 =
                0,                      $ parameter value slot
                6,"20 64 24 B4 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 180",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param181 =
                0,                      $ parameter value slot
                6,"20 64 24 B5 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 181",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param182 =
                0,                      $ parameter value slot
                6,"20 64 24 B6 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 182",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param183 =
                0,                      $ parameter value slot
                6,"20 64 24 B7 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 183",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param184 =
                0,                      $ parameter value slot
                6,"20 64 24 B8 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 184",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param185 =
                0,                      $ parameter value slot
                6,"20 64 24 B9 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 185",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param186 =
                0,                      $ parameter value slot
                6,"20 64 24 BA 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 186",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param187 =
                0,                      $ parameter value slot
                6,"20 64 24 BB 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 187",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param188 =
                0,                      $ parameter value slot
                6,"20 64 24 BC 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 188",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param189 =
                0,                      $ parameter value slot
                6,"20 64 24 BD 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 189",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param190 =
                0,                      $ parameter value slot
                6,"20 64 24 BE 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 190",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param191 =
                0,                      $ parameter value slot
                6,"20 64 24 BF 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 191",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param192 =
                0,                      $ parameter value slot
                6,"20 64 24 C0 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 192",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param193 =
                0,                      $ parameter value slot
                6,"20 64 24 C1 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 193",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param194 =
                0,                      $ parameter value slot
                6,"20 64 24 C2 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 194",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param195 =
                0,                      $ parameter value slot
                6,"20 64 24 C3 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 195",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param196 =
                0,                      $ parameter value slot
                6,"20 64 24 C4 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 196",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param197 =
                0,                      $ parameter value slot
                6,"20 64 24 C5 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 197",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param198 =
                0,                      $ parameter value slot
                6,"20 64 24 C6 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 198",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param199 =
                0,                      $ parameter value slot
                6,"20 64 24 C7 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 199",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param200 =
                0,                      $ parameter value slot
                6,"20 64 24 C8 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 200",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param201 =
                0,                      $ parameter value slot
                6,"20 64 24 C9 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 201",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param202 =
                0,                      $ parameter value slot
                6,"20 64 24 CA 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 202",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param203 =
                0,                      $ parameter value slot
                6,"20 64 24 CB 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 203",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param204 =
                0,                      $ parameter value slot
                6,"20 64 24 CC 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 204",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param205 =
                0,                      $ parameter value slot
                6,"20 64 24 CD 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 205",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param206 =
                0,                      $ parameter value slot
                6,"20 64 24 CE 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 206",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param207 =
                0,                      $ parameter value slot
                6,"20 64 24 CF 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 207",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param208 =
                0,                      $ parameter value slot
                6,"20 64 24 D0 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 208",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param209 =
                0,                      $ parameter value slot
                6,"20 64 24 D1 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 209",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param210 =
                0,                      $ parameter value slot
                6,"20 64 24 D2 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 210",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param211 =
                0,                      $ parameter value slot
                6,"20 64 24 D3 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 211",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param212 =
                0,                      $ parameter value slot
                6,"20 64 24 D4 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 212",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param213 =
                0,                      $ parameter value slot
                6,"20 64 24 D5 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 213",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param214 =
                0,                      $ parameter value slot
                6,"20 64 24 D6 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 214",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param215 =
                0,                      $ parameter value slot
                6,"20 64 24 D7 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 215",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param216 =
                0,                      $ parameter value slot
                6,"20 64 24 D8 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 216",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param217 =
                0,                      $ parameter value slot
                6,"20 64 24 D9 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 217",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param218 =
                0,                      $ parameter value slot
                6,"20 64 24 DA 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 218",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param219 =
                0,                      $ parameter value slot
                6,"20 64 24 DB 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 219",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param220 =
                0,                      $ parameter value slot
                6,"20 64 24 DC 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 220",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param221 =
                0,                      $ parameter value slot
                6,"20 64 24 DD 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 221",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param222 =
                0,                      $ parameter value slot
                6,"20 64 24 DE 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 222",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param223 =
                0,                      $ parameter value slot
                6,"20 64 24 DF 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 223",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param224 =
                0,                      $ parameter value slot
                6,"20 64 24 E0 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 224",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param225 =
                0,                      $ parameter value slot
                6,"20 64 24 E1 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 225",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param226 =
                0,                      $ parameter value slot
                6,"20 64 24 E2 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 226",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param227 =
                0,                      $ parameter value slot
                6,"20 64 24 E3 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 227",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param228 =
                0,                      $ parameter value slot
                6,"20 64 24 E4 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 228",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param229 =
                0,                      $ parameter value slot
                6,"20 64 24 E5 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 229",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param230 =
                0,                      $ parameter value slot
                6,"20 64 24 E6 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 230",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param231 =
                0,                      $ parameter value slot
                6,"20 64 24 E7 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 231",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param232 =
                0,                      $ parameter value slot
                6,"20 64 24 E8 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 232",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param233 =
                0,                      $ parameter value slot
                6,"20 64 24 E9 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 233",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param234 =
                0,                      $ parameter value slot
                6,"20 64 24 EA 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 234",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param235 =
                0,                      $ parameter value slot
                6,"20 64 24 EB 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 235",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param236 =
                0,                      $ parameter value slot
                6,"20 64 24 EC 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 236",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param237 =
                0,                      $ parameter value slot
                6,"20 64 24 ED 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 237",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param238 =
                0,                      $ parameter value slot
                6,"20 64 24 EE 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 238",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision


        Param239 =
                0,                      $ parameter value slot
                6,"20 64 24 EF 30 01",  $ link path size and path
                0x0030,                 $ descriptor: monitor parameter, read only
                0xC4,
                4,                      $ type is DINT, length is 4 byte
                "Motor parameter 239",  $ parameter name
                "",                     $ units string
                "",                     $ help string
                -2147483648,2147483647,0,    $ min, max, default
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,
                0;                      $ scaling links and precision

        Param1000 =
                0,
                ,,
                0x0000,
                0xC7,
                2,
                "Assembly Output Size",
                "",
                "",
                20,20,20,
                ,,,,
                ,,,,
                0;

        Param1001 =
                0,
                ,,
                0x0000,
                0xC7,
                2,
                "Assembly Input Size",
                "",
                "",
                20,20,20,
                ,,,,
                ,,,,
                0;

        Param1002 =
                0,
                ,,
                0x0010,
                0xD3,
                4,
                "Register input data",
                "",
                "Holds data from a register, 32bit size",
                0,0xFFFFFFFF,0,
                ,,,,
                ,,,,
                0;
        Param1003 =
                0,
                ,,
                0x0000,
                0xD3,
                4,
                "Register output data",
                "",
                "Holds data to a register, 32bit size",
                0,0xFFFFFFFF,0,
                ,,,,
                ,,,,
                0;

[Assembly]
        Assem100 =
                " Write Assembly",
                ,
                32,
                0x0000,
                ,,
                32,Param4,
                32,Param4,
                32,Param4,
                32,Param4,
                32,Param4,
                32,Param4,
                32,Param4,
                32,Param4;
        Assem101 =
                " Read Assembly",
                ,
                32,
                0x0000,
                ,,
                32,Param3,
                32,Param3,
                32,Param3,
                32,Param3,
                32,Param3,
                32,Param3,
                32,Param3,
                32,Param3;

[Connection Manager]
        Connection1 =
                0x04010002,             $ Trigger and Transport
                0x44640405,             $ Point Multicast
                ,,Assem100,             $ OT RPI Size format
                ,,Assem101,             $ TO rpi size format
                ,,                      $ config 1
                ,,                      $ config 2
                "Data, In/Out       ",  $ connection name
                "Assembly Object In/Out Data",    $ help string
                "20 04 24 01 2C 64 2C 65";    $ path

        Connection2 =
                0x01010002,             $ Trigger and Transport
                0x44240305,             $ Point Multicast
                ,0,,                    $ OT RPI Size format
                ,,Assem101,             $ TO rpi size format
                ,,                      $ config 1
                ,,                      $ config 2
                "Listen only        ",  $ connection name
                "Assembly Object In/Out Data",    $ help string
                "20 04 24 01 2C C0 2C 65";    $ path

        Connection3 =
                0x02010002,             $ Trigger and Transport
                0x44640305,             $ Point Multicast
                ,0,,                    $ OT RPI Size format
                ,,Assem101,             $ TO rpi size format
                ,,                      $ config 1
                ,,                      $ config 2
                "Input only",           $ connection name
                "Assembly Object In/Out Data",    $ help string
                "20 04 24 01 2C C1 2C 65";    $ path


[Port]
        Port1 =
                TCP,
                "Port 1",
                "20 F5 24 01",
                2;


[Capacity]

        ConnOverhead = .004;            $ Connection Overhead

        MaxIOConnections = 3;           $ Maximum number of Class 1 Connections
        MaxMsgConnections = 6;          $ Maximum number of Class 3 Connections
        TSpec1 = TxRx, 10, 2000;        $ packets per sec @ 10 bytes
        TSpec2 = TxRx, 100, 1500;       $ packets per sec @ 100 bytes

[DLR Class]
        Revision = 2;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;

[Ethernet Link Class]
        Revision = 3;
        MaxInst = 2;
        Number_Of_Static_Instances = 2;
        Max_Number_Of_Dynamic_Instances = 0;
        InterfaceLabel1 = "L/A IN";
        InterfaceLabel2 = "L/A OUT";



$ ****************************************************************************
$ EOF
$ ****************************************************************************
